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R100  低温球阀                       

R100  Cryogenic Ball Valve                       

 R100  低温球阀是我公司针对液化天然气LNG接收站、LNG储罐与运输、空分装置、石油化工尾气分离设备、低温甲醇洗、液氧液氮等低温储槽及槽车等低温超低温工况专门开发的一种切断球阀。

R100 Cryogenic Ball Valve is a kind of cut-off ball valve specially developed by Chongqing Chuanyi Control Valve Co., Ltd. for low-temperature and ultra-low-temperature working conditions such as LNG terminal, LNG storage tank and transportation, ASU (Air Separation Unit), petrochemical tail gas separation equipment, rectisol process, low temperature liquid oxygen and nitrogen storage tank and tanker truck.

R100  低温球阀的设计、制造和检验采用BS6364、SHELL SPE77/200、GB/T24925、ASME16.34等国际通用标准，具有密封性好、可靠性高、使用寿命长等特点。

According to international standards such as BS6364, SHELL SPE77/200, GB/T24925, ASME16.34, R100 Cryogenic Ball Valve is designed, manufactured and tested. It has the characteristics of excellent sealing performance, high reliability and long service life.

产品特点：1、伸长型上阀盖，避免填料冻伤。

Product features: 1. Extensible upper valve cover, avoiding packing damage.

具有定向泄压功能。

2. Directional pressure relief function.
3、防火、防静电功能。

3. Fire prevention, anti-static function.

4、阀杆防飞出结构。

4. Blowout proof stem.

5、可实现双向密封。

5. Two-way sealing.

6、可实现阀门在线维护。

6. Valve maintenance can be carried out without removing the valve from the pipeline.

[image: image7.png]B BN

g




标准规格 

Standard Specifications

型谱Type Spectrum

	产品类型
	Product Type

	低温球阀
	Cryogenic ball valve

	外观型式
	Appearance

	标准
	Standard

	上装
	Top-mounted

	阀座型式
	Valve seat type

	软密封
	Soft seal

	硬密封
	Hard seal

	结构型式
	Structure

	浮动球
	Floating ball valve

	固定球
	Fixed ball valve


系列型号

Model of Series Products

	产品型号

Product Model  
	产品名称

Product Name
	外观型式

Appearance
	阀座型式

Valve Seat Type
	结构型式

Structure

	R100—200
	软密封浮动低温球阀

Soft-Seal Floating Cryogenic Ball Valve
	标准

Standard
	软密封

Soft seal
	浮动球

Floating ball valve

	R100—201
	软密封固定低温球阀

Soft-Seal Fixed Cryogenic Ball Valve
	标准

Standard
	软密封

Soft seal
	固定球

Fixed ball valve

	R100—210
	硬密封浮动低温球阀

Hard-Seal Floating Cryogenic Ball Valve
	标准

Standard
	硬密封

Hard seal
	浮动球

Floating ball valve

	R100—211
	硬密封固定低温球阀

Hard-Seal Fixed Cryogenic Ball Valve
	标准

Standard
	硬密封

Hard seal
	固定球

Fixed ball valve

	R100—300
	上装软密封浮动低温球阀

Top-Mounted Soft-Seal Floating Cryogenic Ball Valve
	上装

Top-mounted
	软密封

Soft seal
	浮动球

Floating ball valve

	R100—301
	上装软密封固定低温球阀

Top-Mounted Soft-Seal Fixed Cryogenic Ball Valve
	上装

Top-mounted
	软密封

Soft seal
	固定球

Fixed ball valve

	R100—310
	上装硬密封浮动低温球阀

Top-mounted Hard-seal Floating Cryogenic Ball Valve
	上装

Top-mounted
	软密封

Soft seal
	浮动球

Floating ball valve

	R100—311
	上装硬密封固定低温球阀

Top-mounted Hard-seal Fixed Cryogenic Ball Valve
	上装

Top-mounted
	软密封

Soft seal
	固定球

Fixed ball valve


阀体 

Valve Body

	形    式  

Type
	直通铸造球型阀 

Through ball valve

	公称通径

Nominal diameter
	1/2"（15）、3/4"（20）、1"（25）、1¼"（32）、1½"（40）、2"（50）、2½"（65）、3"（80）、4"（100）、5"（125）、6"（150）、8"（200）、10"（250）

12"（300）、14"（350）、16"（400）、18"（450）、20"（500）、24"（600）

	公称压力
Nominal pressure
	PN 16、20、25、40、50、63、100、110、150、160、260

Class 150、300、600、900、1500

	连接型式
Connection type
	法兰型：FF、RF、MFM、RJ、BW

Flange type: FF, RF, MFM, RJ, BW

法兰标准：ASME B16.5 ; JIS B2201 ; HG/T 20592 ; HG/T 20615; JB/T 79.1 ; JB/T 79.2 ;

 GB/T 9112

Flange standard: ASME B16.5 ; JIS B2201 ; HG/T 20592 ; HG/T 20615; JB/T 79.1 ; JB/T 79.2 ;

 GB/T 9112

	材   料   

Material
	见表1 

See Table 1

	填    料  

Packing
	石墨填料

Graphite packing


阀内组件 

Valve Subassembly

	阀芯型式

Valve spool type
	球型阀芯 

Ball type valve spool

	流量特性 

Flow characteristics
	快开特性 

Quick opening

	材    料 

Material
	见表1 

See Table 1


执行机构 

Actuator

	          型号 Model

规格 

Specifications
	气动执行机构

Pneumatic actuator

	
	AT  
	AW

	供气压力

Air supply pressure
	400～700kPa

	气源接口

Air source interface
	NPT1/8″、NPT 1/4″、NPT 3/8″、NPT 1/2″、NPT 3/4″

	行程角度

Stroke angle
	90°

90°

	环境温度

Ambient temperature
	标准型 -20～+80℃

Standard type -20～+80℃

高温型 -15～+120℃

High-temperature type -15～+120℃

低温型 -40～+80℃

Low-temperature type  -40～+80℃

	附件

Accessories
	电磁阀、空气过滤减压器、保位阀、行程开关、阀位传送器、手轮机构等

Solenoid valve, air filter pressure reducer, lock-up valve, position limit switch, valve position conveyor, handwheel mechanism, etc.


阀体、阀内零件材料组合及使用温度

Material Combination and Service Temperature of Valve Body and Inner Parts

表1A 浮动球型 （R100—200、R100—210、R100—300）

Table 1A Floating Ball Valve (R100—200, R100—210, R100—300)
·HT：热处理     ·HF：表面硬化处理

HT: Heat Treatment HF: Hard Face

	阀体材料

Body material
	A351-CF8，A351-CF8M，A351-CF3M，A182-F304，A182-F316

	球芯
Ball spool
	材质

Material
	304/316/316L

	
	处理

Processing
	HF 

	阀杆

Valve stem
	材质

Material
	S20910

	
	处理

Processing
	HT

	阀座

Valve seat
	材质

Material
	PCTFE/304/316/316L

	
	处理

Processing
	/HF

	
	不锈钢阀体

Stainless steel valve body
	-196~+150

	阀座允许泄漏量

Allowable leakage of valve seat
	参照BS6364标准规定

Refer to the provisions of BS6364 standard

	阀门密封方向

Valve sealing direction
	单向密封

One-way seal


表1B 固定球型（R100—201、R100—211、R100—301）

Table 1B Fixed Ball Valve (R100—201, R100—211, R100—301)

	阀体材料

Body material
	A351-CF8，A351-CF8M，A351-CF3M，A182-F304，A182-F316

	球芯
Ball spool
	材质

Material
	304/316/316L

	
	处理

Processing
	HF

	阀杆

Valve stem
	材质

Material
	S20910

	
	处理

Processing
	HT

	阀座

Valve seat
	材质

Material
	PCTFE/304/316/316L

	
	处理

Processing
	/HF

	
	不锈钢阀体

Stainless steel valve body
	-196~+150

	阀座允许泄漏量

Allowable leakage of valve seat
	参照BS6364标准规定

Refer to the provisions of BS6364 standard

	阀门密封方向

Valve sealing direction
	双向密封

Two-way seal


表2－1 阀体材料的使用温度·压力范围                                                单位：MPa

Table 2-1 Use Temperature and Pressure Range of Valve Body Materials                       Unit: MPa

	温度

℃

Temperatur (℃)
	Class150
	Class300
	Class600
	Class900
	Class1500

	
	CF8
	CF8M
	CF8
	CF8M
	CF8
	CF8M
	CF8
	CF8M
	CF8
	CF8M

	-254～38
	1.90
	1.90
	4.95
	4.95
	9.93
	9.93
	14.89
	14.89
	24.79
	24.79

	-5～38
	1.90
	1.90
	4.95
	4.95
	9.93
	9.93
	14.89
	14.89
	24.79
	24.79

	50
	1.84
	1.84
	4.77
	4.80
	9.56
	9.62
	14.35
	14.43
	23.90
	24.04

	100
	1.56
	1.61
	4.08
	4.21
	8.17
	8.44
	12.26
	12.66
	20.42
	21.09

	150
	1.39
	1.47
	3.62
	3.85
	7.40
	7.70
	11.10
	11.55
	18.16
	19.24

	200
	1.25
	1.37
	3.27
	3.56
	6.90
	7.13
	10.34
	10.70
	16.37
	17.83

	250
	1.16
	1.20
	3.04
	3.34
	6.50
	6.68
	9.75
	10.01
	15.26
	16.68

	300
	1.01
	1.01
	2.91
	3.15
	6.18
	6.32
	9.27
	9.49
	14.52
	15.80

	350
	0.84
	0.84
	2.81
	3.03
	5.93
	6.07
	8.89
	9.10
	14.02
	15.20

	375
	0.73
	0.73
	2.77
	2.96
	5.81
	5.98
	8.71
	8.96
	13.86
	14.84

	400
	0.64
	0.64
	2.74
	2.91
	5.69
	5.89
	8.53
	8.83
	13.72
	14.55

	425
	0.55
	0.55
	2.71
	2.87
	5.60
	5.83
	8.40
	8.74
	13.57
	14.32

	450
	0.47
	0.47
	2.68
	2.81
	5.48
	5.77
	8.22
	8.65
	13.42
	14.03

	475
	0.37
	0.37
	2.65
	2.73
	5.39
	5.73
	8.08
	8.60
	13.27
	13.67

	500
	0.28
	0.28
	2.60
	2.67
	5.30
	5.65
	7.95
	8.47
	13.02
	13.40

	525
	0.18
	0.18
	2.19
	2.57
	4.89
	5.00
	7.33
	7.52
	11.94
	12.89

	550
	
	
	2.00
	2.40
	4.71
	4.98
	7.07
	7.48
	10.91
	12.48

	566
	
	
	1.90
	2.20
	4.17
	4.79
	6.25
	7.18
	18.16
	19.24


表2-2  JB/T79-94或HG20592-2009

Table 2-2 JB/T79-94 or HG20592-2009

	温度

.℃

Temperature (℃)
	PN16
	PN40
	PN63
	PN100

	
	ZG0Cr18Ni9

	-254～200
	1.60
	4.00
	6.30
	10.0

	～300
	1.40
	3.50
	5.40
	9.00

	～400
	1.20
	3.00
	4.80
	7.50

	～480
	1.10
	2.60
	4.00
	6.60

	～520
	0.90
	2.30
	3.70
	5.80

	～560
	0.80
	2.00
	3.20
	5.00


图1 填料使用温度·压力范围
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Figure 1 Use Temperature·Pressure Range of Packing

图2 垫圈使用温度·压力范围

Figure 2 Use Temperature·Pressure Range of Gasket
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阀体结构

Structure of Valve Body  
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	支架
	Bracket

	压板
	Plate

	压盖
	Gland

	填料
	Packing

	密封圈
	Sealing ring

	阀盖
	Valve cap

	阀杆
	Valve stem

	密封圈
	Sealing ring

	轴承
	Bearing

	右阀体
	Right valve body

	左阀体
	Left valve body

	阀体
	Valve body

	球芯
	Ball spool

	阀座
	Valve seat


图3浮动低温球阀

Figure 3 Floating Cryogenic Ball Valve
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	Bracket

	压板
	Plate

	压盖
	Gland

	填料
	Packing

	密封圈
	Sealing ring

	阀盖
	Valve cap

	阀杆
	Valve stem

	密封圈
	Sealing ring

	轴承
	Bearing

	右阀体
	Right valve body

	左阀体
	Left valve body

	阀体
	Valve body

	球芯
	Ball spool

	阀座
	Valve seat

	弹簧
	Spring

	密封圈
	Sealing ring

	底轴
	Bottom shaft


图4固定低温球阀

Figure 4 Fixed Cryogenic Ball Valve
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	压板
	Plate

	支架
	Bracket

	压盖
	Gland

	垫圈
	Gasket

	密封圈
	Sealing ring

	垫圈
	Gasket

	阀体
	Valve body

	阀座
	Valve seat

	连接件
	Connecting part

	压板
	Plate

	填料
	Packing

	填料函
	Packing box

	阀杆
	Valve stem

	阀盖
	Valve cap

	密封圈
	Sealing ring

	挡圈
	Retainer ring

	阀座
	Valve seat

	球芯
	Ball spool


图5上装浮动低温球阀

Figure 5 Top-Mounted Floating Cryogenic Ball Valve
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	阀杆
	Valve stem

	阀盖
	Valve cap

	密封圈
	Sealing ring

	轴承
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	密封圈
	Sealing ring

	阀座
	Valve seat

	阀体
	Valve body

	弹簧
	Spring

	轴承
	Bearing

	球芯
	Ball spool

	弹簧
	Spring

	阀座
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	密封圈
	Sealing ring


图6上装固定低温球阀

Figure 6 Top-Mounted Fixed Cryogenic Ball Valve

执行机构标准配置及最大关闭压力

Standard Configuration and Maximum Closing Pressure of Actuator 

表3－1低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1 Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)       Unit: MPa

气动双作用执行机构（气开）             气源压力:500kPa

Pneumatic Double Acting Actuator (FC)     Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN16,20/ Class150

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构  

Actuator
	AT63DR0
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT75DR0
	
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT83DR0
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92DR0
	
	
	1.96
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DR0
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DR0
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DR0
	
	
	
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AT160DR0
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	
	
	

	
	AT190DR0
	
	
	
	
	
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	

	
	AT210DR0
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AT240DR0
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	

	
	AT270DR0
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	

	
	AT300DR0
	
	
	
	
	
	
	
	
	
	
	
	
	1.5
	
	
	
	
	

	
	AT350DR0
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	

	
	AT400DR0
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	
	
	
	1.5
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.8
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	1.0

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.5

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.
表3－1（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1 (Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气关）             气源压力:500kPa

Pneumatic Double Acting Actuator (FO)     Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN16,20/ Class150

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构  

Actuator 
	AT63DD0
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT75DD0
	
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT83DD0
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92DD0
	
	
	1.96
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DD0
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DD0
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DD0
	
	
	
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AT160DD0
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	
	
	

	
	AT190DD0
	
	
	
	
	
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	

	
	AT210DD0
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AT240DD0
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	

	
	AT270DD0
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	

	
	AT300DD0
	
	
	
	
	
	
	
	
	
	
	
	
	1.5
	
	
	
	
	

	
	AT350DD0
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	

	
	AT400DD0
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	
	
	
	1.5
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.8
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	1.0

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.5

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－1（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1 (Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气开）            气源压力:500kPa

Pneumatic Double Acting Actuator (FC)    Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN25,40,50/Class300

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT63DR0
	3
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT75DR0
	5
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT83DR0
	
	5
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92DR0
	
	
	5
	3
	1
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DR0
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DR0
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DR0
	
	
	
	
	
	5
	4
	2
	
	
	
	
	
	
	
	
	
	

	
	AT160DR0
	
	
	
	
	
	
	
	5
	1
	
	
	
	
	
	
	
	
	

	
	AT190DR0
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AT210DR0
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	
	

	
	AT240DR0
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	

	
	AT270DR0
	
	
	
	
	
	
	
	
	
	
	5
	2
	1
	
	
	
	
	

	
	AT300DR0
	
	
	
	
	
	
	
	
	
	
	
	3
	1.5
	
	
	
	
	

	
	AT350DR0
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	

	
	AT400DR0
	
	
	
	
	
	
	
	
	
	
	
	
	5
	2
	2
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	
	5
	2
	1
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	
	
	3
	1.4
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	1
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	
	
	5
	2.7
	1.8
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	3
	2
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	1
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	2
	1
	1

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	2.9
	2
	1.5

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	3
	2.7
	2

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	2.9

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	3

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－1（续） 低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气关）             气源压力:500kPa

Pneumatic Double Acting Actuator (FO)     Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN25,40,50/Class300

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT63DD0
	3
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT75DD0
	5
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT83DD0
	
	5
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92DD0
	
	
	5
	3
	1
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DD0
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DD0
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DD0
	
	
	
	
	
	5
	4
	2
	
	
	
	
	
	
	
	
	
	

	
	AT160DD0
	
	
	
	
	
	
	
	5
	1
	
	
	
	
	
	
	
	
	

	
	AT190DD0
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AT210DD0
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	
	

	
	AT240DD0
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	

	
	AT270DD0
	
	
	
	
	
	
	
	
	
	
	5
	2
	1
	
	
	
	
	

	
	AT300DD0
	
	
	
	
	
	
	
	
	
	
	
	3
	1.5
	
	
	
	
	

	
	AT350DD0
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	

	
	AT400DD0
	
	
	
	
	
	
	
	
	
	
	
	
	5
	2
	2
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	
	5
	2
	1
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	
	
	3
	1.4
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	1
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	
	
	5
	2.7
	1.8
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	3
	2
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	1
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	2
	1
	1

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	2.9
	2
	1.5

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	3
	2.7
	2

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	2.9

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	3

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－1（续）低温球阀   软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1(Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气开）             气源压力:500kPa

Pneumatic Double Acting Actuator (FC)     Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN63,100,110/Class600

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT92DR0
	5
	5
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DR0
	7
	7
	7
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DR0
	10
	10
	10
	9
	6
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DR0
	
	
	
	
	10
	9
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DR0
	
	
	
	
	
	10
	8
	5
	
	
	
	
	
	
	
	
	
	

	
	AT190DR0
	
	
	
	
	
	
	10
	9
	5
	
	
	
	
	
	
	
	
	

	
	AT210DR0
	
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	

	
	AT240DR0
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	

	
	AT270DR0
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AT300DR0
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	

	
	AT350DR0
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	

	
	AT400DR0
	
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	9
	6
	
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	10
	9
	
	
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	5.8
	
	
	
	

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	5
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	5
	
	

	
	AW65D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	7
	6
	

	
	AW70D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9
	7
	5

	
	AW75D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	8
	6

	
	AW75D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	8

	
	AW80D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9

	
	AW85D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－1（续）低温球阀   软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)     Unit: MPa

气动双作用执行机构（气关）             气源压力:500kPa

Pneumatic Double Acting Actuator (FO)     Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN63,100,110/Class600

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT92DD0
	5
	5
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DD0
	7
	7
	7
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DD0
	10
	10
	10
	9
	6
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DD0
	
	
	
	
	10
	9
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DD0
	
	
	
	
	
	10
	8
	5
	
	
	
	
	
	
	
	
	
	

	
	AT190DD0
	
	
	
	
	
	
	10
	9
	5
	
	
	
	
	
	
	
	
	

	
	AT210DD0
	
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	

	
	AT240DD0
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	

	
	AT270DD0
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AT300DD0
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	

	
	AT350DD0
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	

	
	AT400DD0
	
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	9
	6
	
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	10
	9
	
	
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	5.8
	
	
	
	

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	5
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	5
	
	

	
	AW65D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	7
	6
	

	
	AW70D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9
	7
	5

	
	AW75D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	8
	6

	
	AW75D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	8

	
	AW80D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9

	
	AW85D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－1（续）低温球阀   软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1(Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)    Unit: MPa

气动双作用执行机构（气开）             气源压力:500kPa

Pneumatic Double Acting Actuator (FC)     Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN150,160/Class900

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT125DR0
	11
	11
	11
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DR0
	15
	15
	15
	15
	11
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DR0
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190DR0
	
	
	
	
	
	15
	14
	
	
	
	
	
	
	
	
	
	
	

	
	AT210DR0
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	

	
	AT240DR0
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	

	
	AT270DR0
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AT300DR0
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	

	
	AT350DR0
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	

	
	AT400DR0
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	

	
	AW18D001
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	10
	
	
	
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	11
	
	
	
	
	

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	

	
	AW65D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	

	
	AW70D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	

	
	AW75D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	11
	
	

	
	AW75D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	13
	10
	

	
	AW80D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	12
	

	
	AW85D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	14
	10

	
	AW90D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	11

	
	AW90D008
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－1（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)     Unit: MPa

气动双作用执行机构（气关）             气源压力:500kPa

Pneumatic Double Acting Actuator (FO)     Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN150,160/Class900

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT125DD0
	11
	11
	11
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DD0
	15
	15
	15
	15
	11
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DD0
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190DD0
	
	
	
	
	
	15
	14
	
	
	
	
	
	
	
	
	
	
	

	
	AT210DD0
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	

	
	AT240DD0
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	

	
	AT270DD0
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AT300DD0
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	

	
	AT350DD0
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	

	
	AT400DD0
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	

	
	AW18D001
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	10
	
	
	
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	11
	
	
	
	
	

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	

	
	AW65D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	

	
	AW70D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	

	
	AW75D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	11
	
	

	
	AW75D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	13
	10
	

	
	AW80D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	12
	

	
	AW85D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	14
	10

	
	AW90D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	11

	
	AW90D008
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－1（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1(Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)    Unit: MPa

气动双作用执行机构（气开）             气源压力:500kPa

Pneumatic Double Acting Actuator (FC)     Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN260/ Class1500

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	
	

	执 行 机 构

Actuator
	AT125DRO
	15.0
	15.0
	15.0
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DRO
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DRO
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	
	

	
	AT190DRO
	
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	

	
	AT210DRO
	
	
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	

	
	AT270DRO
	
	
	
	
	
	
	
	15.0
	13.0
	
	
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	15.0
	15.0
	
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	15.0
	13.0
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	10.0
	
	


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－1（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-1(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)    Unit: MPa

气动双作用执行机构（气关）             气源压力:500kPa

Pneumatic Double Acting Actuator (FO)     Air Source Pressure: 500kPa

	阀体等级

Valve body grade
	PN260/ Class1500

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	
	

	执 行 机 构

Actuator 
	AT125DDO
	15.0
	15.0
	15.0
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DDO
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DDO
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	
	

	
	AT190DDO
	
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	

	
	AT210DDO
	
	
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	

	
	AT270DDO
	
	
	
	
	
	
	
	15.0
	13.0
	
	
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	15.0
	15.0
	
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	15.0
	13.0
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	10.0
	
	


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－2   低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-2  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa
气动单作用执行机构 （气开）            气源压力:500kPa

Pneumatic Single Acting Actuator (FC)      Air Source:500kPa

	阀体等级

Valve body grade
	PN16,20/ Class150

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT83SR5
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92SR5
	
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105SR5
	
	
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SR5
	
	
	1.96
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SR5
	
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SR5
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SR5
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AT210SR5
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	
	
	

	
	AT240SR5
	
	
	
	
	
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	

	
	AT270SR5
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AT300SR5
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AT350SR5
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW18SR51
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	

	
	AW22SR51
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	

	
	AW24SR51
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AW24SR52
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AW27SR52
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AW30SR52
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW32SR52
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	

	
	AW32SR53
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	

	
	AW40SR53
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AW45SR53
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	

	
	AW45SR54
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	

	
	AW50SR54
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.6
	
	
	

	
	AW55SR54
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	

	
	AW60SR55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	1.0
	

	
	AW65SR55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.96
	1.0

	
	AW70SR55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－2（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-2(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa
气动单作用执行机构（气关）             气源压力:500kPa

Pneumatic Single Acting Actuator (FO)      Air Source:500kPa

	阀体等级

Valve body grade
	PN16,20/ Class150

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT83SD5
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92SD5
	
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105SD5
	
	
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SD5
	
	
	1.96
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SD5
	
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SD5
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SD5
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AT210SD5
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	
	
	

	
	AT240SD5
	
	
	
	
	
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	

	
	AT270SD5
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AT300SD5
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AT350SD5
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW18SD51
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	

	
	AW22SD51
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	

	
	AW24SD51
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AW24SD52
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AW27SD52
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AW30SD52
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW32SD52
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	

	
	AW32SD53
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	

	
	AW40SD53
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AW45SD53
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	

	
	AW45SD54
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	

	
	AW50SD54
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.6
	
	
	

	
	AW55SD54
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	

	
	AW60SD55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	1.0
	

	
	AW65SD55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.96
	1.0

	
	AW70SD55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－2（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）
Table 3-2(Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa
气动单作用执行机构 （气开）             气源压力:500kPa

Pneumatic Single Acting Actuator (FC)       Air Source:500kPa

	阀体等级

Valve body grade
	PN25,40,50/Class300

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT83SR5
	3
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92SR5
	5
	2
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105SR5
	
	5
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SR5
	
	
	5
	3
	1
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SR5
	
	
	
	
	5
	3
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SR5
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SR5
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	
	
	

	
	AT210SR5
	
	
	
	
	
	
	
	5
	1
	
	
	
	
	
	
	
	
	

	
	AT240SR5
	
	
	
	
	
	
	
	
	4
	2
	
	
	
	
	
	
	
	

	
	AT270SR5
	
	
	
	
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	

	
	AT300SR5
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AT350SR5
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	

	
	AW18SR51
	
	
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	

	
	AW22SR51
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	
	

	
	AW24SR51
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AW24SR52
	
	
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	
	
	

	
	AW27SR52
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AW30SR52
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	

	
	AW32SR52
	
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	

	
	AW32SR53
	
	
	
	
	
	
	
	
	
	
	
	2.9
	1
	
	
	
	
	

	
	AW35SR53
	
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	

	
	AW40SR53
	
	
	
	
	
	
	
	
	
	
	
	4
	1.9
	
	
	
	
	

	
	AW45SR53
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	

	
	AW45SR54
	
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	1
	
	
	

	
	AW50SR54
	
	
	
	
	
	
	
	
	
	
	
	
	5
	2.5
	1.6
	
	
	

	
	AW55SR54
	
	
	
	
	
	
	
	
	
	
	
	
	
	3
	2
	
	
	

	
	AW55SR55
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	
	
	

	
	AW60SR55
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	1
	1
	

	
	AW65SR55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	4.7
	2
	2
	1

	
	AW70SR55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	3
	2


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－2（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）
Table 3-2(Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa
气动单作用执行机构 （气关）              气源压力:500kPa

Pneumatic Single Acting Actuator (FO)       Air Source:500kPa

	阀体等级

Valve body grade
	PN25,40,50/Class300

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT83SD5
	3
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92SD5
	5
	2
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105SD5
	
	5
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SD5
	
	
	5
	3
	1
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SD5
	
	
	
	
	5
	3
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SD5
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SD5
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	
	
	

	
	AT210SD5
	
	
	
	
	
	
	
	5
	1
	
	
	
	
	
	
	
	
	

	
	AT240SD5
	
	
	
	
	
	
	
	
	4
	2
	
	
	
	
	
	
	
	

	
	AT270SD5
	
	
	
	
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	

	
	AT300SD5
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AT350SD5
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	

	
	AW18SD51
	
	
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	

	
	AW22SD51
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	
	

	
	AW24SD51
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AW24SD52
	
	
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	
	
	

	
	AW27SD52
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AW30SD52
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	

	
	AW32SD52
	
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	

	
	AW32SD53
	
	
	
	
	
	
	
	
	
	
	
	2.9
	1
	
	
	
	
	

	
	AW35SD53
	
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	

	
	AW40SD53
	
	
	
	
	
	
	
	
	
	
	
	4
	1.9
	
	
	
	
	

	
	AW45SD53
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	

	
	AW45SD54
	
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	1
	
	
	

	
	AW50SD54
	
	
	
	
	
	
	
	
	
	
	
	
	5
	2.5
	1.6
	
	
	

	
	AW55SD54
	
	
	
	
	
	
	
	
	
	
	
	
	
	3
	2
	
	
	

	
	AW55SD55
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	
	
	

	
	AW60SD55
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	1
	1
	

	
	AW65SD55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	4.7
	2
	2
	1

	
	AW70SD55
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	3
	2


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－2（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）
Table 3-2(Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa
气动单作用执行机构 （气开）              气源压力:500kPa

Pneumatic Single Acting Actuator (FC)       Air Source:500kPa

	阀体等级

Valve body grade
	PN63,100,110/Class600

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT125SR5
	5
	5
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SR5
	9
	9
	9
	7
	5
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SR5
	10
	10
	10
	10
	8
	6
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SR5
	
	
	
	
	10
	10
	5
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SR5
	
	
	
	
	
	
	8
	5
	
	
	
	
	
	
	
	
	
	

	
	AT240SR5
	
	
	
	
	
	
	10
	9
	
	
	
	
	
	
	
	
	
	

	
	AT270SR5
	
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	

	
	AT300SR5
	
	
	
	
	
	
	
	
	9
	6
	
	
	
	
	
	
	
	

	
	AT350SR5
	
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	

	
	AW18SR51
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	
	
	

	
	AW22SR51
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	
	

	
	AW24SR51
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	

	
	AW24SR52
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	
	
	

	
	AW27SR52
	
	
	
	
	
	
	
	
	8.7
	5
	
	
	
	
	
	
	
	

	
	AW30SR52
	
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	

	
	AW32SR52
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AW32SR53
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	
	
	
	

	
	AW35SR53
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	
	

	
	AW40SR53
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	

	
	AW45SR53
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	

	
	AW45SR54
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	

	
	AW50SR54
	
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	

	
	AW55SR54
	
	
	
	
	
	
	
	
	
	
	
	10
	5.8
	
	
	
	
	

	
	AW55SR55
	
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	

	
	AW60SR55
	
	
	
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	

	
	AW65SR55
	
	
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	

	
	AW70SR55
	
	
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	

	
	AW80SR56
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	9
	6
	5
	3

	
	AW85SR56
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	7
	6
	4


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－2（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-2(Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa
气动单作用执行机构 （气关）              气源压力:500kPa

Pneumatic Single Acting Actuator (FO)       Air Source:500kPa

	阀体等级

Valve body grade
	PN63,100,110/Class600

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT125SD5
	5
	5
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SD5
	9
	9
	9
	7
	5
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SD5
	10
	10
	10
	10
	8
	6
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SD5
	
	
	
	
	10
	10
	5
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SD5
	
	
	
	
	
	
	8
	5
	
	
	
	
	
	
	
	
	
	

	
	AT240SD5
	
	
	
	
	
	
	10
	9
	
	
	
	
	
	
	
	
	
	

	
	AT270SD5
	
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	

	
	AT300SD5
	
	
	
	
	
	
	
	
	9
	6
	
	
	
	
	
	
	
	

	
	AT350SD5
	
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	

	
	AW18SD51
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	
	
	

	
	AW22SD51
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	
	

	
	AW24SD51
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	

	
	AW24SD52
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	
	
	

	
	AW27SD52
	
	
	
	
	
	
	
	
	8.7
	5
	
	
	
	
	
	
	
	

	
	AW30SD52
	
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	

	
	AW32SD52
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AW32SD53
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	
	
	
	

	
	AW35SD53
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	
	

	
	AW40SD53
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	

	
	AW45SD53
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	

	
	AW45SD54
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	

	
	AW50SD54
	
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	

	
	AW55SD54
	
	
	
	
	
	
	
	
	
	
	
	10
	5.8
	
	
	
	
	

	
	AW55SD55
	
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	

	
	AW60SD55
	
	
	
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	

	
	AW65SD55
	
	
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	

	
	AW70SD55
	
	
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	

	
	AW80SD56
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	9
	6
	5
	3

	
	AW85SD56
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	7
	6
	4


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.
表3－2（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）
Table 3-2(Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa
气动单作用执行机构 （气开）             气源压力:500kPa

Pneumatic Single Acting Actuator (FC)       Air Source:500kPa

	阀体等级

Valve body grade
	PN150,160/Class900

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT160SR5
	15
	15
	15
	13
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SR5
	
	
	
	15
	12
	10
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SR5
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT240SR5
	
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	
	

	
	AT270SR5
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	
	

	
	AT300SR5
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	
	
	
	

	
	AT350SR5
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	
	
	

	
	AW18SR51
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	
	
	
	

	
	AW22SR51
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	
	

	
	AW24SR51
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	
	

	
	AW24SR52
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	
	
	

	
	AW27SR52
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	
	
	

	
	AW30SR52
	
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	

	
	AW32SR52
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AW32SR53
	
	
	
	
	
	
	
	
	
	11
	
	
	
	
	
	
	
	

	
	AW35SR53
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	

	
	AW40SR53
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	

	
	AW45SR53
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	

	
	AW45SR54
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	

	
	AW50SR54
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	

	
	AW55SR54
	
	
	
	
	
	
	
	
	
	
	
	10
	
	
	
	
	
	

	
	AW55SR55
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	

	
	AW60SR55
	
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	

	
	AW65SR55
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	

	
	AW70SR55
	
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	

	
	AW80SR56
	
	
	
	
	
	
	
	
	
	
	
	
	15
	14
	9
	6
	5
	3

	
	AW85SR56
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	7
	6
	4


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－2（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）
Table 3-2(Contd) Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa
气动单作用执行机构 （气关）              气源压力:500kPa

Pneumatic Single Acting Actuator (FO)       Air Source:500kPa

	阀体等级

Valve body grade
	PN150,160/Class900

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT160SD5
	15
	15
	15
	13
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SD5
	
	
	
	15
	12
	10
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SD5
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT240SD5
	
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	
	

	
	AT270SD5
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	
	

	
	AT300SD5
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	
	
	
	

	
	AT350SD5
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	
	
	

	
	AW18SD51
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	
	
	
	

	
	AW22SD51
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	
	

	
	AW24SD51
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	
	

	
	AW24SD52
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	
	
	

	
	AW27SD52
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	
	
	

	
	AW30SD52
	
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	

	
	AW32SD52
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AW32SD53
	
	
	
	
	
	
	
	
	
	11
	
	
	
	
	
	
	
	

	
	AW35SD53
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	

	
	AW40SD53
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	

	
	AW45SD53
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	

	
	AW45SD54
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	

	
	AW50SD54
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	

	
	AW55SD54
	
	
	
	
	
	
	
	
	
	
	
	10
	
	
	
	
	
	

	
	AW55SD55
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	

	
	AW60SD55
	
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	

	
	AW65SD55
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	

	
	AW70SD55
	
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	

	
	AW80SD56
	
	
	
	
	
	
	
	
	
	
	
	
	15
	14
	9
	6
	5
	3

	
	AW85SD56
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	7
	6
	4


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－2（续）   低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）

Table 3-2 (Contd) Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)

气动单作用执行机构 （气开）             气源压力:500kPa

Pneumatic Single Acting Actuator (FC)      Air Source:500kPa

	阀体等级

Valve body grade
	PN260/ Class1500

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	
	

	执 行 机 构

Actuator 
	AT160SR5
	15.0
	15.0
	15.0
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SR5
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SR5
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	
	

	
	AT240SR5
	
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	

	
	AT270SR5
	
	
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	

	
	AW40SR53
	
	
	
	
	
	
	
	15.0
	11.0
	
	
	
	
	
	
	

	
	AW45SR53
	
	
	
	
	
	
	
	
	15.0
	15.0
	
	
	
	
	
	

	
	AW55SR55
	
	
	
	
	
	
	
	
	
	
	15.0
	
	
	
	
	

	
	AW65SR55
	
	
	
	
	
	
	
	
	
	
	
	13.0
	8.0
	4.9
	
	


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－2 （续）   低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）

Table 3-2 (Contd) Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)

气动单作用执行机构 （气关）            气源压力:500kPa

Pneumatic Single Acting Actuator (FO)     Air Source:500kPa

	阀体等级

Valve body grade
	PN260/ Class1500

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	
	

	执 行 机 构

Actuator 
	AT160SD5
	15.0
	15.0
	15.0
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SD5
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SD5
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	
	

	
	AT240SD5
	
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	
	

	
	AT270SD5
	
	
	
	
	
	
	15.0
	
	
	
	
	
	
	
	
	

	
	AW40SD53
	
	
	
	
	
	
	
	15.0
	11.0
	
	
	
	
	
	
	

	
	AW45SD53
	
	
	
	
	
	
	
	
	15.0
	15.0
	
	
	
	
	
	

	
	AW55SD55
	
	
	
	
	
	
	
	
	
	
	15.0
	
	
	
	
	

	
	AW65SD55
	
	
	
	
	
	
	
	
	
	
	
	13.0
	8.0
	4.9
	
	


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－3 低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-3  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气开）             气源压力:400kPa

Pneumatic Double Acting Actuator (FC)     Air Source Pressure: 400kPa

	阀体等级

Valve body grade
	PN16,20/ Class150

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT63DR0
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT75DR0
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT83DR0
	
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92DR0
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DR0
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DR0
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DR0
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	

	
	AT160DR0
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AT190DR0
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	

	
	AT210DR0
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AT240DR0
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AT270DR0
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AT300DR0
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	

	
	AT350DR0
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AT400DR0
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	1.0
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－3（续） 低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-3(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气关）             气源压力:400kPa

Pneumatic Double Acting Actuator (FO)     Air Source Pressure: 400kPa

	阀体等级

Valve body grade
	PN16,20/ Class150

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT63DD0
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT75DD0
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT83DD0
	
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92DD0
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DD0
	
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DD0
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DD0
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	

	
	AT160DD0
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AT190DD0
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	

	
	AT210DD0
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AT240DD0
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AT270DD0
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AT300DD0
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	

	
	AT350DD0
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AT400DD0
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	1.0
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－3（续） 低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-3(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气开）             气源压力:400kPa

Pneumatic Double Acting Actuator (FC)     Air Source Pressure: 400kPa

	阀体等级

Valve body grade
	PN25,40,50/Class300

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	
	AT63DR0
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT75DR0
	4
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT83DR0
	5
	3
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	执 行 机 构

Actuator 
	AT92DR0
	
	5
	3
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DR0
	
	
	5
	4
	2
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DR0
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DR0
	
	
	
	
	
	5
	2
	1
	
	
	
	
	
	
	
	
	
	

	
	AT160DR0
	
	
	
	
	
	
	5
	3
	
	
	
	
	
	
	
	
	
	

	
	AT190DR0
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	
	

	
	AT210DR0
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AT240DR0
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AT270DR0
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	

	
	AT300DR0
	
	
	
	
	
	
	
	
	
	
	5
	2
	1
	
	
	
	
	

	
	AT350DR0
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	
	
	
	
	

	
	AT400DR0
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	1
	1
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	5
	4
	2
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	
	4
	2
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	
	5
	2.3
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	1
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	2
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	1
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	1.96
	1
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	2
	1

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	2


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－3（续） 低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-3(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气关）             气源压力:400kPa

Pneumatic Double Acting Actuator (FO)     Air Source Pressure: 400kPa

	阀体等级

Valve body grade
	PN25,40,50/Class300

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	
	AT63DD0
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT75DD0
	4
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT83DD0
	5
	3
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	执 行 机 构

Actuator 
	AT92DD0
	
	5
	3
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT105DD0
	
	
	5
	4
	2
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DD0
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DD0
	
	
	
	
	
	5
	2
	1
	
	
	
	
	
	
	
	
	
	

	
	AT160DD0
	
	
	
	
	
	
	5
	3
	
	
	
	
	
	
	
	
	
	

	
	AT190DD0
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	
	

	
	AT210DD0
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AT240DD0
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AT270DD0
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	

	
	AT300DD0
	
	
	
	
	
	
	
	
	
	
	5
	2
	1
	
	
	
	
	

	
	AT350DD0
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	
	
	
	
	

	
	AT400DD0
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	1
	1
	
	
	

	
	AW18D001
	
	
	
	
	
	
	
	5
	4
	2
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	
	4
	2
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	
	5
	2.3
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	1
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	2
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	1
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	1.96
	1
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	2
	1

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	2


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－3（续）低温球阀 软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-3(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气开）             气源压力:400kPa

Pneumatic Double Acting Actuator (FC)     Air Source Pressure: 400kPa

	阀体等级

Valve body grade
	PN63,100,110/Class600

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT105DR0
	5
	5
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DR0
	9
	9
	9
	7
	5
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DR0
	10
	10
	10
	10
	9
	6
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DR0
	
	
	
	
	10
	10
	6
	
	
	
	
	
	
	
	
	
	
	

	
	AT190DR0
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	
	

	
	AT210DR0
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	
	
	
	
	

	
	AT240DR0
	
	
	
	
	
	
	
	10
	8
	5
	
	
	
	
	
	
	
	

	
	AT270DR0
	
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	

	
	AT300DR0
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AT350DR0
	
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	
	
	

	
	AT400DR0
	
	
	
	
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	

	
	AW18D001
	
	
	
	
	
	
	10
	9
	
	
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	5
	
	
	

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	

	
	AW65D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	6
	5
	

	
	AW70D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	7
	6
	

	
	AW75D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	7
	5

	
	AW75D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	8
	6

	
	AW80D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9
	7

	
	AW85D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	8

	
	AW90D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9

	
	AW90D008
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－3（续）低温球阀 软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-3(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气关）             气源压力:400kPa

Pneumatic Double Acting Actuator (FO)     Air Source Pressure: 400kPa

	阀体等级

Valve body grade
	PN63,100,110/Class600

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT105DD0
	5
	5
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125DD0
	9
	9
	9
	7
	5
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140DD0
	10
	10
	10
	10
	9
	6
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DD0
	
	
	
	
	10
	10
	6
	
	
	
	
	
	
	
	
	
	
	

	
	AT190DD0
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	
	

	
	AT210DD0
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	
	
	
	
	

	
	AT240DD0
	
	
	
	
	
	
	
	10
	8
	5
	
	
	
	
	
	
	
	

	
	AT270DD0
	
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	

	
	AT300DD0
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AT350DD0
	
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	
	
	

	
	AT400DD0
	
	
	
	
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	

	
	AW18D001
	
	
	
	
	
	
	10
	9
	
	
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	5
	
	
	

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	

	
	AW65D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	6
	5
	

	
	AW70D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	7
	6
	

	
	AW75D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	8
	7
	5

	
	AW75D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	8
	6

	
	AW80D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9
	7

	
	AW85D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	8

	
	AW90D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9

	
	AW90D008
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	10


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－3（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-3(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气开）             气源压力:400kPa

Pneumatic Double Acting Actuator (FC)     Air Source Pressure: 400kPa

	阀体等级

Valve body grade
	PN150,160/Class900

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT140DR0
	15
	15
	15
	14
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DR0
	
	
	
	15
	14
	11
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190DR0
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	
	

	
	AT210DR0
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	
	
	
	

	
	AT240DR0
	
	
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	

	
	AT270DR0
	
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	

	
	AT300DR0
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AT350DR0
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	
	

	
	AT400DR0
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	

	
	AW18D001
	
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	11
	
	
	
	
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	10
	
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	

	
	AW65D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	

	
	AW70D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	

	
	AW75D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	

	
	AW75D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	

	
	AW80D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	

	
	AW85D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	14
	11
	

	
	AW90D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	12
	

	
	AW90D008
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	12


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－3（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-3(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动双作用执行机构（气关）             气源压力:400kPa

Pneumatic Double Acting Actuator (FO)     Air Source Pressure: 400kPa

	阀体等级

Valve body grade
	PN150,160/Class900

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator
	AT140DD0
	15
	15
	15
	14
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160DD0
	
	
	
	15
	14
	11
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190DD0
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	
	

	
	AT210DD0
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	
	
	
	

	
	AT240DD0
	
	
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	

	
	AT270DD0
	
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	

	
	AT300DD0
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AT350DD0
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	
	

	
	AT400DD0
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	

	
	AW18D001
	
	
	
	
	
	15
	13
	
	
	
	
	
	
	
	
	
	
	

	
	AW22D001
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	
	

	
	AW22D002
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	

	
	AW24D002
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	
	

	
	AW27D002
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AW27D003
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	

	
	AW30D003
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	
	

	
	AW32D003
	
	
	
	
	
	
	
	
	
	
	11
	
	
	
	
	
	
	

	
	AW35D003
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	

	
	AW35D004
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	

	
	AW40D004
	
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	

	
	AW45D004
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	

	
	AW50D004
	
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	

	
	AW50D005
	
	
	
	
	
	
	
	
	
	
	
	
	10
	
	
	
	
	

	
	AW55D005
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	

	
	AW60D005
	
	
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	

	
	AW65D005
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	

	
	AW65D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	

	
	AW70D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	

	
	AW75D006
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	

	
	AW75D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	

	
	AW80D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	12
	
	

	
	AW85D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	14
	11
	

	
	AW90D007
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	12
	

	
	AW90D008
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	15
	12


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－4   低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-4  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动单作用执行机构 （气开）                气源压力:400kPa

Pneumatic Single Acting Actuator (FC)         Air Source:400kPa

	阀体等级

Valve body grade
	PN16,20/ Class150

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT83SR4
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92SR4
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SR4
	
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SR4
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SR4
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SR4
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SR4
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	

	
	AT210SR4
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AT240SR4
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	

	
	AT270SR4
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AT300SR4
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AT350SR4
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW18SR41
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AW22SR41
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	
	
	

	
	AW24SR41
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	

	
	AW24SR42
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AW27SR42
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AW30SR42
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AW32SR42
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW32SR43
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	

	
	AW40SR43
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	

	
	AW45SR43
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AW45SR44
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	

	
	AW50SR44
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	

	
	AW55SR45
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	

	
	AW65SR45
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	10.
	

	
	AW70SR45
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0

	
	AW80SR46
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－4（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-4(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动单作用执行机构（气关）                气源压力:400kPa

Pneumatic Single Acting Actuator (FO)        Air Source:400kPa

	阀体等级

Valve body grade
	PN16,20/ Class150

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT83SD4
	1.0
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92SD4
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SD4
	
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SD4
	
	
	1.96
	1.96
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SD4
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SD4
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SD4
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	
	
	

	
	AT210SD4
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AT240SD4
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	

	
	AT270SD4
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AT300SD4
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AT350SD4
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW18SD41
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	
	
	

	
	AW22SD41
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	
	
	

	
	AW24SD41
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	
	
	
	
	
	

	
	AW24SD42
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	
	

	
	AW27SD42
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	
	

	
	AW30SD42
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	
	

	
	AW32SD42
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	
	

	
	AW32SD43
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	
	

	
	AW40SD43
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	
	

	
	AW45SD43
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	
	
	

	
	AW45SD44
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	
	
	
	

	
	AW50SD44
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0
	
	
	

	
	AW55SD45
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	
	
	

	
	AW65SD45
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.0
	10.
	

	
	AW70SD45
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96
	1.0

	
	AW80SD46
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	1.96


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－4（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-4(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动单作用执行机构 （气开）              气源压力:400kPa

Pneumatic Single Acting Actuator (FC)       Air Source:400kPa

	阀体等级

Valve body grade
	PN25,40,50/Class300

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT83SR4
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92SR4
	4
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SR4
	5
	3
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SR4
	
	5
	3
	2
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SR4
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SR4
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SR4
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	
	
	
	

	
	AT210SR4
	
	
	
	
	
	
	5
	3
	
	
	
	
	
	
	
	
	
	

	
	AT240SR4
	
	
	
	
	
	
	
	5
	2
	1
	
	
	
	
	
	
	
	

	
	AT270SR4
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AT300SR4
	
	
	
	
	
	
	
	
	
	4
	2
	
	
	
	
	
	
	

	
	AT350SR4
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	

	
	AW18SR41
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	
	
	

	
	AW22SR41
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	
	
	
	
	

	
	AW24SR41
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	
	

	
	AW24SR42
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AW27SR42
	
	
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	
	
	

	
	AW30SR42
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AW32SR42
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	

	
	AW32SR43
	
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	

	
	AW40SR43
	
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	

	
	AW45SR43
	
	
	
	
	
	
	
	
	
	
	
	4
	1.96
	
	
	
	
	

	
	AW45SR44
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	

	
	AW50SR44
	
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	1
	
	
	

	
	AW55SR45
	
	
	
	
	
	
	
	
	
	
	
	
	
	3
	2
	
	
	

	
	AW60SR45
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	
	
	

	
	AW65SR45
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	1
	1
	

	
	AW70SR45
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	4.7
	2
	2
	1

	
	AW80SR46
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	4
	3


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－4（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-4(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动单作用执行机构（气关）               气源压力:400kPa

Pneumatic Single Acting Actuator (FO)       Air Source:400kPa

	阀体等级

Valve body grade
	PN25,40,50/Class300

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT83SD4
	1
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT92SD4
	4
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SD4
	5
	3
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT125SD4
	
	5
	3
	2
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT140SD4
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SD4
	
	
	
	
	5
	4
	1
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SD4
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	
	
	
	

	
	AT210SD4
	
	
	
	
	
	
	5
	3
	
	
	
	
	
	
	
	
	
	

	
	AT240SD4
	
	
	
	
	
	
	
	5
	2
	1
	
	
	
	
	
	
	
	

	
	AT270SD4
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AT300SD4
	
	
	
	
	
	
	
	
	
	4
	2
	
	
	
	
	
	
	

	
	AT350SD4
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	

	
	AW18SD41
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	
	
	

	
	AW22SD41
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	
	
	
	
	

	
	AW24SD41
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	
	
	
	
	

	
	AW24SD42
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	
	

	
	AW27SD42
	
	
	
	
	
	
	
	
	
	4
	1
	
	
	
	
	
	
	

	
	AW30SD42
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	
	

	
	AW32SD42
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	
	

	
	AW32SD43
	
	
	
	
	
	
	
	
	
	
	5
	2
	
	
	
	
	
	

	
	AW40SD43
	
	
	
	
	
	
	
	
	
	
	
	3
	1
	
	
	
	
	

	
	AW45SD43
	
	
	
	
	
	
	
	
	
	
	
	4
	1.96
	
	
	
	
	

	
	AW45SD44
	
	
	
	
	
	
	
	
	
	
	
	5
	3
	1
	
	
	
	

	
	AW50SD44
	
	
	
	
	
	
	
	
	
	
	
	
	4
	2
	1
	
	
	

	
	AW55SD45
	
	
	
	
	
	
	
	
	
	
	
	
	
	3
	2
	
	
	

	
	AW60SD45
	
	
	
	
	
	
	
	
	
	
	
	
	
	4
	3
	
	
	

	
	AW65SD45
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	1
	1
	

	
	AW70SD45
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	4.7
	2
	2
	1

	
	AW80SD46
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	5
	4
	4
	3


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－4（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-4(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动单作用执行机构 （气开）              气源压力:400kPa

Pneumatic Single Acting Actuator (FC)       Air Source:400kPa

	阀体等级

Valve body grade
	PN63,100,110/Class600

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT140SR4
	7
	7
	7
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SR4
	10
	10
	10
	9
	6
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SR4
	
	
	
	10
	10
	7
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SR4
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	
	
	

	
	AT240SR4
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	
	

	
	AT270SR4
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	
	
	

	
	AT300SR4
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	
	
	

	
	AT350SR4
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	

	
	AW18SR41
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	
	
	
	
	

	
	AW22SR41
	
	
	
	
	
	
	7
	
	
	
	
	
	
	
	
	
	
	

	
	AW24SR41
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	
	

	
	AW24SR42
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	

	
	AW27SR42
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	
	
	

	
	AW30SR42
	
	
	
	
	
	
	
	
	8.7
	5
	
	
	
	
	
	
	
	

	
	AW32SR42
	
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	

	
	AW32SR43
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AW35SR43
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	
	
	
	

	
	AW40SR43
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	
	

	
	AW45SR43
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	

	
	AW45SR44
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	

	
	AW50SR44
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	

	
	AW55SR44
	
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	

	
	AW55SR45
	
	
	
	
	
	
	
	
	
	
	
	10
	5.8
	
	
	
	
	

	
	AW60SR45
	
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	

	
	AW65SR45
	
	
	
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	

	
	AW70SR45
	
	
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	

	
	AW80SR46
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	7
	5
	4
	

	
	AW85SR46
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9
	6
	5
	3


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－4（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-4(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动单作用执行机构（气关）               气源压力:400kPa

Pneumatic Single Acting Actuator (FO)       Air Source:400kPa

	阀体等级

Valve body grade
	PN63,100,110/Class600

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT140SD4
	7
	7
	7
	5
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT160SD4
	10
	10
	10
	9
	6
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SD4
	
	
	
	10
	10
	7
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SD4
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	
	
	

	
	AT240SD4
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	
	

	
	AT270SD4
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	
	
	

	
	AT300SD4
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	
	
	

	
	AT350SD4
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	

	
	AW18SD41
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	
	
	
	
	

	
	AW22SD41
	
	
	
	
	
	
	7
	
	
	
	
	
	
	
	
	
	
	

	
	AW24SD41
	
	
	
	
	
	
	10
	7
	
	
	
	
	
	
	
	
	
	

	
	AW24SD42
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	
	
	
	

	
	AW27SD42
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	
	
	

	
	AW30SD42
	
	
	
	
	
	
	
	
	8.7
	5
	
	
	
	
	
	
	
	

	
	AW32SD42
	
	
	
	
	
	
	
	
	10
	8
	
	
	
	
	
	
	
	

	
	AW32SD43
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	
	
	
	

	
	AW35SD43
	
	
	
	
	
	
	
	
	
	
	6
	
	
	
	
	
	
	

	
	AW40SD43
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	
	

	
	AW45SD43
	
	
	
	
	
	
	
	
	
	
	8
	
	
	
	
	
	
	

	
	AW45SD44
	
	
	
	
	
	
	
	
	
	
	10
	6
	
	
	
	
	
	

	
	AW50SD44
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	
	

	
	AW55SD44
	
	
	
	
	
	
	
	
	
	
	
	9
	5
	
	
	
	
	

	
	AW55SD45
	
	
	
	
	
	
	
	
	
	
	
	10
	5.8
	
	
	
	
	

	
	AW60SD45
	
	
	
	
	
	
	
	
	
	
	
	
	7
	
	
	
	
	

	
	AW65SD45
	
	
	
	
	
	
	
	
	
	
	
	
	9
	
	
	
	
	

	
	AW70SD45
	
	
	
	
	
	
	
	
	
	
	
	
	10
	5
	
	
	
	

	
	AW80SD46
	
	
	
	
	
	
	
	
	
	
	
	
	
	10
	7
	5
	4
	

	
	AW85SD46
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	9
	6
	5
	3


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－4（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-4(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动单作用执行机构 （气开）              气源压力:400kPa

Pneumatic Single Acting Actuator (FC)       Air Source:400kPa

	阀体等级

Valve body grade
	PN150,160/Class900

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT160SR4
	11
	11
	11
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SR4
	15
	15
	15
	15
	10
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SR4
	
	
	
	
	14
	11
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT240SR4
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	
	

	
	AT270SR4
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	
	

	
	AT300SR4
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	
	
	
	

	
	AT350SR4
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	

	
	AW18SR41
	
	
	
	15
	13
	10
	
	
	
	
	
	
	
	
	
	
	
	

	
	AW22SR41
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	
	
	
	

	
	AW24SR41
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	
	

	
	AW24SR42
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	
	

	
	AW27SR42
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	
	
	

	
	AW30SR42
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	
	
	

	
	AW32SR42
	
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	

	
	AW32SR43
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AW35SR43
	
	
	
	
	
	
	
	
	
	11
	
	
	
	
	
	
	
	

	
	AW40SR43
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	

	
	AW45SR43
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	

	
	AW45SR44
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	

	
	AW50SR44
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	

	
	AW55SR44
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	

	
	AW55SR45
	
	
	
	
	
	
	
	
	
	
	
	10
	
	
	
	
	
	

	
	AW60SR45
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	

	
	AW65SR45
	
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	

	
	AW70SR45
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	

	
	AW80SR46
	
	
	
	
	
	
	
	
	
	
	
	
	15
	12
	7
	5
	4
	

	
	AW85SR46
	
	
	
	
	
	
	
	
	
	
	
	
	
	14
	9
	6
	5
	3


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.

表3－4（续）低温球阀  软密封（R100—200、R100—201、R100—300、R100—301）最大关闭压力（单位：MPa）

Table 3-4(Contd)  Maximum Closing Pressure of Soft-Seal Cryogenic Ball Valve (R100—200, R100—201, R100—300, R100—301)      Unit: MPa

气动单作用执行机构（气关）               气源压力:400kPa

Pneumatic Single Acting Actuator (FO)       Air Source:400kPa

	阀体等级

Valve body grade
	PN150,160/Class900

	公称通径

Nominal diameter

Inch (mm)
	1/2"

(15)
	3/4"

(20)
	1"

(25)
	1¼"

(32)
	1½"

(40)
	2"

(50)
	2½"

(65)
	3"

(80)
	4"

(100)
	5"

(125)
	6"

(150)
	8"

(200)
	10"

(250)
	12"

(300)
	14"

(350)
	16"

(400)
	18"

(450)
	20"

(500)

	执 行 机 构

Actuator 
	AT160SD4
	11
	11
	11
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT190SD4
	15
	15
	15
	15
	10
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT210SD4
	
	
	
	
	14
	11
	
	
	
	
	
	
	
	
	
	
	
	

	
	AT240SD4
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	
	

	
	AT270SD4
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	
	

	
	AT300SD4
	
	
	
	
	
	
	
	12
	
	
	
	
	
	
	
	
	
	

	
	AT350SD4
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	

	
	AW18SD41
	
	
	
	15
	13
	10
	
	
	
	
	
	
	
	
	
	
	
	

	
	AW22SD41
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	
	
	
	

	
	AW24SD41
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	
	
	
	
	

	
	AW24SD42
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	
	
	

	
	AW27SD42
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	
	
	

	
	AW30SD42
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	
	
	

	
	AW32SD42
	
	
	
	
	
	
	
	15
	12
	
	
	
	
	
	
	
	
	

	
	AW32SD43
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	
	
	
	

	
	AW35SD43
	
	
	
	
	
	
	
	
	
	11
	
	
	
	
	
	
	
	

	
	AW40SD43
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	
	

	
	AW45SD43
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	
	
	

	
	AW45SD44
	
	
	
	
	
	
	
	
	
	15
	11
	
	
	
	
	
	
	

	
	AW50SD44
	
	
	
	
	
	
	
	
	
	
	13
	
	
	
	
	
	
	

	
	AW55SD44
	
	
	
	
	
	
	
	
	
	
	15
	
	
	
	
	
	
	

	
	AW55SD45
	
	
	
	
	
	
	
	
	
	
	
	10
	
	
	
	
	
	

	
	AW60SD45
	
	
	
	
	
	
	
	
	
	
	
	12
	
	
	
	
	
	

	
	AW65SD45
	
	
	
	
	
	
	
	
	
	
	
	14
	
	
	
	
	
	

	
	AW70SD45
	
	
	
	
	
	
	
	
	
	
	
	15
	10
	
	
	
	
	

	
	AW80SD46
	
	
	
	
	
	
	
	
	
	
	
	
	15
	12
	7
	5
	4
	

	
	AW85SD46
	
	
	
	
	
	
	
	
	
	
	
	
	
	14
	9
	6
	5
	3


注：最大允许压差不准超过ASME B16.34标准规定。

Note: The maximum allowable pressure difference shall not exceed the value specified in standard ASME B16.34.
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图7 R100标准式浮动球阀配AW和AT气动执行机构（R100—200、R100—210）

Figure 7 R100 Standard Floating Ball Valve with AW and AT Pneumatic Actuator (R100—200,R100—210)
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图8. R100标准式固定球阀配AW和AT气动执行机构（R100—201、R100—211）

Figure 8 R100 Standard Fixed Ball Valve with AW and AT Pneumatic Actuator (R100—201, R100—211)
外形尺寸及重量 

Overall Dimensions and Weight

（注：如下述表格中数据与技术提供的外形尺寸图数据不一致时，以外形尺寸图数据为准）

(Note: In case of inconsistency between the data in the following tables and the dimension drawing data provided by the technology department, the dimension drawing data shall prevail)
表4-1 标准式低温球阀 PN16/Class150配气动执行机构外形尺寸及重量（R100—200、R100—210、R100—201、R100—211）                                                                             mm

Table 4-1 Overall Dimensions and Weight of Standard Cryogenic Ball Valve PN16/Class150 with Pneumatic Actuator (R100—200, R100—210, R100—201, R100—211)                                    mm
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT125SR5

AT125SD5
	537
	350
	
	
	108
	55
	
	4" (100)
	AT240SR5

AT240SD5
	869
	620
	
	
	229
	136
	

	
	AT83DRO

AT83DDO
	450
	235
	
	
	
	
	
	
	AT190DRO

AT190DDO
	810
	540
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27SR52 AW27SD52
	924
	
	650
	950
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW22D001
	864
	
	520
	200
	
	
	

	3/4" (20)
	AT125SR5

AT125SD5
	537
	350
	
	
	117
	55
	
	5" (125)
	AT270SR5

AT270SD5
	958
	740
	
	
	356
	157
	

	
	AT83DRO

AT83DDO
	450
	235
	
	
	
	
	
	
	AT240DRO

AT240DDO
	920
	620
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	974
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	974
	
	650
	250
	
	
	

	1" (25)
	AT125SR5

AT125SD5
	537
	350
	
	
	127
	55
	
	6" (150)
	AT270DRO

AT270DDO
	1034
	740
	
	
	394
	196
	

	
	AT83DRO

AT83DDO
	450
	235
	
	
	
	
	
	
	AW32SR53 AW32SD53
	1049
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1145
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	1049
	
	650
	250
	
	
	

	1¼" (32)
	AT140SR5

AT140SD5
	592
	405
	
	
	140
	65
	
	8" (200)
	AW27D002
	1198
	
	650
	250
	457
	250
	

	
	AT105DRO

AT105DDO
	553
	285
	
	
	
	
	
	
	AW45SR53

AW45SD53
	1417
	
	700
	1250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1320
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW30D003
	1223
	
	700
	270
	
	
	

	1½" (40)
	AT140SR5

AT140SD5
	601
	405
	
	
	165
	70
	
	10"(250)
	AW45SR53

AW45SD53
	1472
	
	700
	1250
	533
	325
	

	
	AT125DRO

AT125DDO
	585
	350
	
	
	
	
	
	
	AW35D004
	1470
	
	800
	320
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW30D003
	1373
	
	700
	270
	
	
	

	2" (50)
	AT160SR5

AT160SD5
	647
	470
	
	
	178
	84
	
	12"(300)
	AW35D004
	1570
	
	800
	320
	610
	380
	

	
	AT125DRO

AT125DDO
	605
	350
	
	
	
	
	
	
	AW55SR55

AW55SD55
	1795
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	724
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	2½" (65)
	AT190SR5

AT190SD5
	710
	540
	
	
	190
	99
	
	14"(350)
	AW35D004
	1810
	
	800
	320
	686
	438
	

	
	AT140DRO

AT140DDO
	642
	405
	
	
	
	
	
	
	AW55D005
	1805
	
	850
	370
	
	
	

	
	AW22SR51 AW22SD51
	744
	
	520
	910
	
	
	
	
	AW55SR55

AW55SD55
	1968
	
	950
	1600
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2018
	
	950
	1600
	
	
	

	3" (80)
	AT210SR5

AT210SD5
	815
	560
	
	
	203
	116
	
	16"(400)
	AW55D005
	2072
	
	950
	370
	762
	440
	

	
	AT160DRO

AT160DDO
	747
	470
	
	
	
	
	
	
	AW60D005
	2070
	
	950
	370
	
	
	

	
	AW27SR52 AW27SD52
	904
	
	650
	950
	
	
	
	
	AW65SR55

AW65SD55
	2118
	
	950
	1600
	
	
	


注：1.本表外形尺寸不包含附件。

Note: 1. The overall dimensions of this table do not include the dimensions of accessories.

表4-2 标准式低温球阀 PN40/Class300配气动执行机构外形尺寸及重量（R100—200、R100—210、R100—201、R100—211）                                                                             mm

Table 4-2 Overall Dimensions and Weight of Standard Cryogenic Ball Valve PN40/Class300 with Pneumatic Actuator (R100—200, R100—210, R100—201, R100—211)                                    mm
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT125SR5

AT125SD5
	495
	350
	
	
	140
	62.5
	
	4" (100)
	AT270SR5

AT270SD5
	908
	740
	
	
	305
	136
	

	
	AT92DRO

AT92DDO
	456
	275
	
	
	
	
	
	
	AT210DRO

AT210DDO
	835
	560
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW22D001
	864
	
	520
	200
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	964
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27SR52 AW27SD52
	924
	
	650
	950
	
	
	

	3/4" (20)
	AT125SR5

AT125SD5
	495
	350
	
	
	152
	62.5
	
	5" (125)
	AT240DRO

AT240DDO
	919
	620
	
	
	381
	157
	

	
	AT92DRO

AT92DDO
	456
	275
	
	
	
	
	
	
	AW27D002
	974
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1009
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	974
	
	700
	1160
	
	
	

	1" (25)
	AT125SR5

AT125SD5
	495
	350
	
	
	165
	62.5
	
	6" (150)
	AW30D003
	1048
	
	700
	270
	403
	196
	

	
	AT92DRO

AT92DDO
	456
	275
	
	
	
	
	
	
	AT270DRO

AT270DDO
	1033
	740
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	1023
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1145
	
	700
	1160
	
	
	

	1¼" (32)
	AT140SR5

AT140SD5
	592
	405
	
	
	178
	65
	
	8" (200)
	AW30D003
	1224
	
	700
	270
	502
	250
	

	
	AT125DRO

AT125DDO
	578
	350
	
	
	
	
	
	
	AW35D004
	1320
	
	800
	320
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW45SR53

AW45SD53
	1322
	
	700
	1250
	
	
	

	1½" (40)
	AT160SR5

AT160SD5
	617
	470
	
	
	190
	70
	
	10"(250)
	AW55SR55

AW55SD55
	1606
	
	950
	1600
	568
	3325
	

	
	AT140DRO

AT140DDO
	592
	405
	
	
	
	
	
	
	AW35D004
	1470
	
	800
	320
	
	
	

	2" (50)
	AT190SR5

AT190SD5
	670
	540
	
	
	216
	85
	
	12"(300)
	AW55D005
	1705
	
	950
	370
	648
	380
	

	
	AT140DRO

AT140DDO
	601
	405
	
	
	
	
	
	
	AW65SR55

AW65SD55
	1868
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	724
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	2½" (65)
	AT210SR5

AT210SD5
	735
	560
	
	
	241
	105
	
	14"(350)
	AW60D005
	1993
	
	950
	370
	762
	438
	

	
	AT160DRO

AT160DDO
	667
	470
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2018
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	764
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	3" (80)
	AT190DRO

AT190DDO
	770
	540
	
	
	\283
	116


	
	16"(400)
	AW60D005
	2093
	
	950
	370
	838
	440
	

	
	AT210SR5

AT210SD5
	795
	560
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2118
	
	950
	1600
	
	
	

	
	AT240SR5

AT240SD5
	829
	620
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AW27SR52 AW27SD52
	884
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	


注：1.本表外形尺寸不包含附件。

Note: 1. The overall dimensions of this table do not include the dimensions of accessories.

表4-3 标准式低温球阀 PN63配气动执行机构外形尺寸及重量（R100—200、R100—210、R100—201、

R100—211）                                                                             mm

Table 4-9 Overall Dimensions and Weight of Standard Cryogenic Ball Valve PN63 with Pneumatic Actuator (R100—200, R100—210, R100—201, R100—211)                                    mm

	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT140SR5

AT140SD5
	542
	405
	
	
	165
	60
	
	4" (100)
	AT270SR5

AT270SD5
	1099
	740
	
	
	406
	181
	

	
	AT92DRO

AT92DDO
	486
	275
	
	
	
	
	
	
	AT210DRO

AT210DDO
	1026
	560
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	1115
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	1115
	
	700
	1160
	
	
	

	3/4" (20)
	AT140SR5

AT140SD5
	542
	405
	
	
	190
	60
	
	5" (125)
	AT240DRO

AT240DDO
	1169
	620
	
	
	457
	245
	

	
	AT92DRO

AT92DDO
	486
	275
	
	
	
	
	
	
	AW27D002
	1224
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1320
	
	700
	1160
	
	
	

	1" (25)
	AT140SR5

AT140SD5
	582
	405
	
	
	216
	70
	
	6" (150)
	AW30D003
	1289
	
	700
	270
	495
	254
	

	
	AT92DRO

AT92DDO
	526
	275
	
	
	
	
	
	
	AW45SR53

AW45SD53
	1388
	
	700
	1250
	
	
	

	1¼" (32)
	AT160SR5

AT160SD5
	669
	470
	
	
	229
	87
	
	8" (200)
	AW35D004
	1450
	
	800
	320
	597
	305
	

	
	AT105DRO

AT105DDO
	605
	285
	
	
	
	
	
	
	AW55SR55

AW55SD55
	1675
	
	950
	1600
	
	
	

	1½" (40)
	AT160SR5

AT160SD5
	705
	470
	
	
	241
	106
	
	10"(250)
	AW35D004
	1612
	
	800
	320
	673
	3336
	

	
	AT140DRO

AT140DDO
	683
	405
	
	
	
	
	
	
	AW65SR55

AW65SD55
	1910
	
	950
	1600
	
	
	

	2" (50)
	AT190SR5

AT190SD5
	768
	540
	
	
	292
	106
	
	12"(300)
	AW55D005
	1932
	
	950
	370
	762
	427
	

	
	AT140DRO

AT140DDO
	700
	405
	
	
	
	
	
	
	AW65SR55

AW65SD55
	1978
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	822
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	2½" (65)
	AT210SR5

AT210SD5
	875
	560
	
	
	330
	134
	
	14"(350)
	AW60D005
	2143
	
	950
	370
	826
	463
	

	
	AT160DRO

AT160DDO
	807
	470
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2168
	
	950
	1600
	
	
	

	
	AW27SR52 AW27SD52
	964
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	

	3" (80)
	AT190DRO

AT190DDO
	941
	540
	
	
	\356
	144


	
	16"(400)
	AW60D005
	2346
	
	950
	370
	902
	541
	

	
	AT240SR5

AT240SD5
	1000
	620
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2371
	
	950
	1600
	
	
	

	
	AW27SR52 AW27SD52
	1032
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	


注：1.本表外形尺寸不包含附件。

Note: 1. The overall dimensions of this table do not include the dimensions of accessories.

表4-4 标准式低温球阀 PN100/Class600配气动执行机构外形尺寸及重量（R100—200、R100—210、

R100—201、R100—211）                                                                   mm

Table 4-4 Overall Dimensions and Weight of Standard Cryogenic Ball Valve PN100/Class600 with Pneumatic Actuator (R100—200, R100—210, R100—201, R100—211)                                    mm
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT140SR5

AT140SD5
	542
	405
	
	
	165
	60
	
	4" (100)
	AT270SR5

T270SD5
	1099
	740
	
	
	432
	181
	

	
	AT92DRO

AT92DDO
	486
	275
	
	
	
	
	
	
	AT210DRO

AT210DDO
	1026
	560
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	1115
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	1115
	
	700
	1160
	
	
	

	3/4" (20)
	AT140SR5

AT140SD5
	542
	405
	
	
	190
	60
	
	5" (125)
	AT240DRO

AT240DDO
	1169
	620
	
	
	508
	245
	

	
	AT92DRO

AT92DDO
	486
	275
	
	
	
	
	
	
	AW27D002
	1224
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1320
	
	700
	1160
	
	
	

	1" (25)
	AT140SR5

AT140SD5
	582
	405
	
	
	216
	70
	
	6" (150)
	AW30D003
	1289
	
	700
	270
	559
	254
	

	
	AT92DRO

AT92DDO
	526
	275
	
	
	
	
	
	
	AW45SR53

AW45SD53
	1388
	
	700
	1250
	
	
	

	1¼" (32)
	AT160SR5

AT160SD5
	669
	470
	
	
	229
	87
	
	8" (200)
	AW35D004
	1450
	
	800
	320
	660
	305
	

	
	AT105DRO

AT105DDO
	605
	285
	
	
	
	
	
	
	AW55SR55

AW55SD55
	1675
	
	950
	1600
	
	
	

	1½" (40)
	AT160SR5

AT160SD5
	705
	470
	
	
	241
	106
	
	10"(250)
	AW35D004
	1612
	
	800
	320
	787
	3336
	

	
	AT140DRO

AT140DDO
	683
	405
	
	
	
	
	
	
	AW65SR55

AW65SD55
	1910
	
	950
	1600
	
	
	

	2" (50)
	AT190SR5

AT190SD5
	768
	540
	
	
	292
	106
	
	12"(300)
	AW55D005
	1932
	
	950
	370
	838
	427
	

	
	AT140DRO

AT140DDO
	700
	405
	
	
	
	
	
	
	AW65SR55

AW65SD55
	1978
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	822
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	2½" (65)
	AT210SR5

AT210SD5
	875
	560
	
	
	330
	134
	
	14"(350)
	AW60D005
	2143
	
	950
	370
	889
	463
	

	
	AT160DRO

AT160DDO
	807
	470
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2168
	
	950
	1600
	
	
	

	
	AW27SR52 AW27SD52
	964
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	

	3" (80)
	AT190DRO

AT190DDO
	941
	540
	
	
	\356
	144


	
	16"(400)
	AW60D005
	2346
	
	950
	370
	991
	541
	

	
	AT240SR5

AT240SD5
	1000
	620
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2371
	
	950
	1600
	
	
	

	
	AW27SR52 AW27SD52
	1032
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	


注：1.本表外形尺寸不包含附件。

Note: 1. The overall dimensions of this table do not include the dimensions of accessories.

表4-5 标准式低温球阀 PN150/Class900配气动执行机构外形尺寸及重量  （R100—200、R100—210、R100—201、R100—211）                                                                    mm

Table 4-5 Overall Dimensions and Weight of Standard Cryogenic Ball Valve PN150/Class900 with Pneumatic Actuator (R100—200, R100—210, R100—201, R100—211)                                    mm

	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT140SR5

AT140SD5
	572
	405
	
	
	254
	65
	
	4" (100)
	AT240DRO

AT240DDO
	1199
	620
	
	
	457
	183
	

	
	AT105DRO

AT105DDO
	533
	285
	
	
	
	
	
	
	AT270SR5

AT270SD5
	1238
	740
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	1253
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	1254
	
	650
	250
	
	
	

	3/4" (20)
	AT140SR5

AT140SD5
	572
	405
	
	
	254
	65
	
	5" (125)
	AT240DRO

AT240DDO
	1349
	620
	
	
	559
	250
	

	
	AT105DRO

AT105DDO
	533
	285
	
	
	
	
	
	
	AW27D002
	1324
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1420
	
	700
	1160
	
	
	

	1" (25)
	AT140SR5

AT140SD5
	622
	405
	
	
	254
	75
	
	6" (150)
	AW30D003
	1343
	
	700
	270
	610
	260
	

	
	AT105DRO

AT105DDO
	566
	285
	
	
	
	
	
	
	AW45SR53

AW45SD53
	1442
	
	700
	1250
	
	
	

	1¼" (32)
	AT160SR5

AT160SD5
	727
	470
	
	
	279
	90
	
	8" (200)
	AW35D004
	1470
	
	800
	320
	737
	310
	

	
	AT125DRO

AT125DDO
	685
	285
	
	
	
	
	
	
	AW55SR55

AW55SD55
	1695
	
	950
	1600
	
	
	

	1½" (40)
	AT190SR5

AT190SD5
	810
	540
	
	
	305
	110
	
	10"(250)
	AW55D005
	1845
	
	950
	370
	838
	3380
	

	
	AT140DRO

AT140DDO
	742
	405
	
	
	
	
	
	
	AW65SR55

AW65SD55
	1918
	
	950
	1600
	
	
	

	2" (50)
	AT210SR5

AT210SD5
	915
	560
	
	
	368
	140
	
	12"(300)
	AW60D005
	1963
	
	950
	370
	965
	420
	

	
	AT160DRO

AT160DDO
	847
	470
	
	
	
	
	
	
	AW65SR55

AW65SD55
	1988
	
	950
	1600
	
	
	

	2½" (65)
	AT240SR5

AT240SD5
	1009
	620
	
	
	419
	150
	
	14"(350)
	AW60D005
	2196
	
	950
	370
	1029
	460
	

	
	AT190DRO

AT190DDO
	950
	540
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2221
	
	950
	1600
	
	
	

	3" (80)
	AT210DRO

AT210DDO
	1115
	560
	
	
	\381
	160


	
	16"(400)
	AW60D005
	2346
	
	950
	370
	1130
	460
	

	
	AW27SR52 AW27SD52
	1204
	
	650
	950
	
	
	
	
	AW65SR55

AW65SD55
	2371
	
	950
	1600
	
	
	

	
	AT270SR5

AT270SD5
	1188
	740
	
	
	
	
	
	
	
	
	
	
	
	
	
	


注：1.本表外形尺寸不包含附件。

Note: 1. The overall dimensions of this table do not include the dimensions of accessories.

表中结构长度A为RF法兰连接形式。如选RJ法兰连接形式时结构长度A请详询技术部。

2. The structural length A in the table is RF flange connection. Please consult the technology department in detail about the structural length A of RJ flange connection.

表4-6 标准体低温球阀 PN260 / Class1500配气动执行机构外形尺寸及重量（R100—200、R100—210、R100—201、R100—211）                                                                     mm

Table 4-6 Overall Dimensions and Weight of Standard Cryogenic Ball Valve PN260 / Class1500 with Pneumatic Actuator (R100—200, R100—210, R100—201, R100—211)                                    mm

	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	法兰式A

Flange A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT125DRO、AT125DDO
	528
	350
	
	
	257
	84
	

	
	AT160SR5、

AT160SD5
	560
	470
	
	
	
	
	

	3/4" (20)
	AT125DRO、AT125DDO
	528
	350
	
	
	257
	84
	

	
	AT160SR5、

AT160SD5
	560
	470
	
	
	
	
	

	1" (25)
	AT125DRO、AT125DDO
	528
	350
	
	
	257
	84
	

	
	AT160SR5、

AT160SD5
	560
	470
	
	
	
	
	

	1¼" (32)
	AT140DRO、AT140DDO
	603
	405
	
	
	282
	91
	

	
	AT190SR5、

AT190SD5
	658
	540
	
	
	
	
	

	1½" (40)
	AT160DRO、AT160DDO
	640
	470
	
	
	308
	94
	

	
	AT210SR5、

AT210SD5
	700
	560
	
	
	
	
	

	2" (50)
	AT240SR5

AT240SD5
	1015
	620
	
	
	371
	190
	

	
	AT190DRO

AT190DDO
	947
	540
	
	
	
	
	

	2½" (65)
	AT270SR5

AT270SD5
	1109
	740
	
	
	422
	200
	

	
	AT210DRO

AT210DDO
	1050
	560
	
	
	
	
	

	3" (80)
	AT270DRO

AT270DDO
	1215
	740
	
	
	473
	210
	

	
	AW40SR53

AW40SD53
	1373
	
	700
	1160
	
	
	

	4" (100)
	AW40SR53

AW40SD53
	1403
	
	700
	1160
	549
	233
	

	
	AT270DRO

AT270DDO
	1336
	740
	
	
	
	
	

	
	AW45SR53

AW45SD53


	1450
	
	700
	1250
	
	
	

	6" (150)
	AW55SR55

AW55SD55
	1595
	
	950
	1600
	711
	310
	

	
	AW35D004
	1540
	
	800
	320
	
	
	

	8" (200)
	AW65SR55

 AW65SD55
	1574
	
	950
	1600
	841
	360
	

	
	AW55D005
	1795
	
	950
	370
	
	
	

	10"(250)
	AW65SR55

AW65SD55
	1811
	
	950
	1600
	1000
	430
	

	
	AW55D005
	2071
	
	950
	370
	
	
	

	12"(300)
	AW65SR55

AW65SD55
	2007
	
	950
	1600
	1146
	471
	

	
	AW60D005
	2077
	
	950
	370
	
	
	


注：1.本表外形尺寸不包含附件。

Note: 1. The overall dimensions of this table do not include the dimensions of accessories.

2.表中结构长度A为RJ法兰连接形式。

2. The structural length A in the table is RF flange connection. 



图9. R100上装式固定球阀配AW和AT气动执行机构外形尺寸（R100—300、R100—301）

Figure 9. Overall Dimensions of R100 Top-mounted Fixed Ball Valve with AW and AT Pneumatic Actuator (R100—300, R100—301)
表4-7 上装式低温球阀 PN16/Class150配气动执行机构外形尺寸及重量（R100—300、R100—301）   mm

Table 4-7 Overall Dimensions and Weight of Top-mounted Cryogenic Ball Valve PN16/Class150 with Pneumatic Actuator (R100—300, R100—301)                                    mm 

	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT125SR5

AT125SD5
	537
	350
	
	
	365
	55
	
	4" (100)
	AT240SR5

AT240SD5
	869
	620
	
	
	632
	143
	

	
	AT83DRO AT83DDO
	450
	235
	
	
	
	
	
	
	AT190DRO

AT190DDO
	810
	540
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27SR52 AW27SD52
	924
	
	650
	950
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW22D001
	864
	
	520
	200
	
	
	

	3/4" (20)
	AT125SR5

AT125SD5
	537
	350
	
	
	390
	
	
	5" (125)
	AT270SR5

AT270SD5
	958
	740
	
	
	708
	157
	

	
	AT83DRO

AT83DDO
	450
	235
	
	
	
	
	
	
	AT240DRO

AT240DDO
	920
	620
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	974
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	974
	
	650
	250
	
	
	

	1" (25)
	AT125SR5

AT125SD5
	537
	350
	
	
	416
	
	
	6" (150)
	AT270DRO

AT270DDO
	1024
	740
	
	
	759
	217
	

	
	AT83DRO

AT83DDO
	450
	235
	
	
	
	
	
	
	AW27D002
	1049
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	1049
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1145
	
	700
	1160
	
	
	

	1¼" (32)
	AT140SR5

AT140SD5
	592
	405
	
	
	429
	65
	
	8" (200)
	AW27D002
	1198
	
	650
	250
	1060
	265
	

	
	AT105DRO

AT105DDO
	553
	285
	
	
	
	
	
	
	AW30D003
	1223
	
	700
	270
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1320
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW45SR53

AW45SD53
	1322
	
	700
	1250
	
	
	

	1½" (40)
	AT140SR5

AT140SD5
	601
	405
	
	
	441
	70
	
	10"(250)
	AW30D003
	1373
	
	700
	270
	1187
	313
	

	
	AT125DRO

AT125DDO
	585
	350
	
	
	
	
	
	
	AW35D004
	1470
	
	800
	320
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW45SR53

AW45SD53
	1567
	
	700
	1250
	
	
	

	2" (50)
	AT160SR5

AT160SD5
	647
	470
	
	
	492
	83
	
	12"(300)
	AW35D004
	1570
	
	800
	320
	1238
	400
	

	
	AT125DRO

AT125DDO
	605
	350
	
	
	
	
	
	
	AW55SR55

AW55SD55
	1795
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	724
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	2½" (65)
	AT190SR5

AT190SD5
	710
	540
	
	
	530
	83
	
	14"(350)
	AW35D004
	1810
	
	800
	320
	1289
	430
	

	
	AT140DRO

AT140DDO
	642
	405
	
	
	
	
	
	
	AW55D005
	1805
	
	850
	370
	
	
	

	
	AW22SR51 AW22SD51
	744
	
	520
	910
	
	
	
	
	AW55SR55

AW55SD55
	1968
	
	950
	1600
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2018
	
	950
	1600
	
	
	

	3" (80)
	AT210SR5

AT210SD5
	815
	560
	
	
	556
	110
	
	16"(400)
	AW55D005
	2072
	
	950
	370
	1391
	452
	

	
	AT160DRO

AT160DDO
	747
	470
	
	
	
	
	
	
	AW60D005
	2070
	
	950
	370
	
	
	

	
	AW27SR52 AW27SD52
	904
	
	650
	950
	
	
	
	
	AW65SR55

AW65SD55
	2118
	
	950
	1600
	
	
	


注：结构长度A已包含袖管尺寸。

Note: Structure length A has included the sleeve size.

表4-8 上装式低温球阀 PN40/Class300配气动执行机构外形尺寸及重量（R100—300、R100—301） mm

Table 4-8 Overall Dimensions and Weight of Top-mounted Cryogenic Ball Valve PN40/Class300 with Pneumatic Actuator (R100—300, R100—301)                                    mm 

	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT125SR5

AT125SD5
	495
	350
	
	
	365
	58
	
	4" (100)
	AT270SR5

AT270SD5
	908
	740
	
	
	632
	143
	

	
	AT92DRO

AT92DDO
	456
	275
	
	
	
	
	
	
	AT210DROAT210DDO
	835
	560
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW22D001
	864
	
	520
	200
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	964
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27SR52 AW27SD52
	924
	
	650
	950
	
	
	

	3/4" (20)
	AT125SR5

AT125SD5
	495
	350
	
	
	390
	
	
	5" (125)
	AT240DROAT240DDO
	919
	620
	
	
	708
	157
	

	
	AT92DRO

AT92DDO
	456
	275
	
	
	
	
	
	
	AW27D002
	974
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1009
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	974
	
	700
	1160
	
	
	

	1" (25)
	AT125SR5

AT125SD5
	495
	350
	
	
	416
	
	
	6" (150)
	AW30D003
	1048
	
	700
	270
	759
	217
	

	
	AT92DRO

AT92DDO
	456
	275
	
	
	
	
	
	
	AT270DROAT270DDO
	1033
	740
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	1023
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1145
	
	700
	1160
	
	
	

	1¼" (32)
	AT140SR5

AT140SD5
	592
	405
	
	
	429
	65
	
	8" (200)
	AW30D003
	1224
	
	700
	270
	1060
	265
	

	
	AT125DRO

AT125DDO
	578
	350
	
	
	
	
	
	
	AW35D004
	1320
	
	800
	320
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW45SR53、AW45SD53
	1322
	
	700
	1250
	
	
	

	1½" (40)
	AT160SR5

AT160SD5
	617
	470
	
	
	441
	70
	
	10"(250)
	AW55SR55、AW55SD55
	1606
	
	950
	1600
	1187
	313
	

	
	AT140DRO

AT140DDO
	592
	405
	
	
	
	
	
	
	AW35D004
	1470
	
	800
	320
	
	
	

	2" (50)
	AT190SR5

AT190SD5
	670
	540
	
	
	492
	83
	
	12"(300)
	AW55D005
	1705
	
	950
	370
	1238
	400
	

	
	AT140DRO

AT140DDO
	601
	405
	
	
	
	
	
	
	AW65SR55、AW65SD55
	1868
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	724
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	2½" (65)
	AT210SR5

AT210SD5
	735
	560
	
	
	530
	83
	
	14"(350)
	AW60D005
	1993
	
	950
	370
	1289
	430
	

	
	AT160DRO

AT160DDO
	667
	470
	
	
	
	
	
	
	AW65SR55、AW65SD55
	2018
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	764
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	3" (80)
	AT190DRO

AT190DDO
	770
	540
	
	
	\556
	110


	
	16"(400)
	AW60D005
	2093
	
	950
	370
	1391
	452
	

	
	AT210SR5

AT210SD5
	795
	560
	
	
	
	
	
	
	AW65SR55、AW65SD55
	2118
	
	950
	1600
	
	
	

	
	AT240SR5

AT240SD5
	829
	620
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	
	AW27SR52 AW27SD52
	884
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	


注：结构长度A已包含袖管尺寸。

Note: Structure length A has included the sleeve size.

表4-9上装式低温球阀 PN63配气动执行机构外形尺寸及重量（R100—300、R100—301）   mm

Table 4-9 Overall Dimensions and Weight of Top-mounted Cryogenic Ball Valve PN63 with Pneumatic Actuator (R100—300, R100—301)                                    mm 

	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT140SR5

AT140SD5
	542
	405
	
	
	365
	60
	
	4" (100)
	AT270SR5

AT270SD5
	1099
	740
	
	
	632
	181
	

	
	AT92DRO

AT92DDO
	486
	275
	
	
	
	
	
	
	AT210DROAT210DDO
	1026
	560
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	1115
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	1115
	
	700
	1160
	
	
	

	3/4" (20)
	AT140SR5

AT140SD5
	542
	405
	
	
	390
	60
	
	5" (125)
	AT240DROAT240DDO
	1169
	620
	
	
	708
	245
	

	
	AT92DRO

AT92DDO
	486
	275
	
	
	
	
	
	
	AW27D002
	1224
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1320
	
	700
	1160
	
	
	

	1" (25)
	AT140SR5

AT140SD5
	582
	405
	
	
	416
	70
	
	6" (150)
	AW30D003
	1289
	
	700
	270
	759
	254
	

	
	AT92DRO

AT92DDO
	526
	275
	
	
	
	
	
	
	AW45SR53AW45SD53
	1388
	
	700
	1250
	
	
	

	1¼" (32)
	AT160SR5

AT160SD5
	669
	470
	
	
	429
	87
	
	8" (200)
	AW35D004
	1450
	
	800
	320
	1060
	305
	

	
	AT105DRO

AT105DDO
	605
	285
	
	
	
	
	
	
	AW55SR55AW55SD55
	1675
	
	950
	1600
	
	
	

	1½" (40)
	AT160SR5

AT160SD5
	705
	470
	
	
	441
	106
	
	10"(250)
	AW35D004
	1612
	
	800
	320
	1187
	336
	

	
	AT140DRO

AT140DDO
	683
	405
	
	
	
	
	
	
	AW65SR55AW65SD55
	1910
	
	950
	1600
	
	
	

	2" (50)
	AT190SR5

AT190SD5
	768
	540
	
	
	492
	106
	
	12"(300)
	AW55D005
	1932
	
	950
	370
	1238
	427
	

	
	AT140DRO

AT140DDO
	700
	405
	
	
	
	
	
	
	AW65SR55AW65SD55
	1978
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	822
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	2½" (65)
	AT210SR5

AT210SD5
	875
	560
	
	
	530
	134
	
	14"(350)
	AW60D005
	2143
	
	950
	370
	1289
	463
	

	
	AT160DRO

AT160DDO
	807
	470
	
	
	
	
	
	
	AW65SR55AW65SD55
	2168
	
	950
	1600
	
	
	

	
	AW27SR52 AW27SD52
	964
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	

	3" (80)
	AT190DRO

AT190DDO
	941
	540
	
	
	\556
	144


	
	16"(400)
	AW60D005
	2346
	
	950
	370
	1391
	541
	

	
	AT240SR5

AT240SD5
	1000
	620
	
	
	
	
	
	
	AW65SR55AW65SD55
	2371
	
	950
	1600
	
	
	

	
	AW27SR52 AW27SD52
	1032
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	


注：结构长度A已包含袖管尺寸。

Note: Structure length A has included the sleeve size.

表4-10上装式低温球阀 PN100/Class600配气动执行机构外形尺寸及重量 （R100—300、R100—301）   mm

Table 4-10 Overall Dimensions and Weight of Top-mounted Cryogenic Ball Valve PN100/Class600 with Pneumatic Actuator (R100—300, R100—301)                                    mm 

	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT140SR5

AT140SD5
	542
	405
	
	
	365
	60
	
	4" (100)
	AT270SR5

AT270SD5
	1099
	740
	
	
	632
	181
	

	
	AT92DRO

AT92DDO
	486
	275
	
	
	
	
	
	
	AT210DROAT210DDO
	1026
	560
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	1115
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	1115
	
	700
	1160
	
	
	

	3/4" (20)
	AT140SR5

AT140SD5
	542
	405
	
	
	390
	60
	
	5" (125)
	AT240DROAT240DDO
	1169
	620
	
	
	708
	245
	

	
	AT92DRO

AT92DDO
	486
	275
	
	
	
	
	
	
	AW27D002
	1224
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1320
	
	700
	1160
	
	
	

	1" (25)
	AT140SR5

AT140SD5
	582
	405
	
	
	416
	70
	
	6" (150)
	AW30D003
	1289
	
	700
	270
	759
	254
	

	
	AT92DRO

AT92DDO
	526
	275
	
	
	
	
	
	
	AW45SR53AW45SD53
	1388
	
	700
	1250
	
	
	

	1¼" (32)
	AT160SR5

AT160SD5
	669
	470
	
	
	429
	87
	
	8" (200)
	AW35D004
	1450
	
	800
	320
	1060
	305
	

	
	AT105DRO

AT105DDO
	605
	285
	
	
	
	
	
	
	AW55SR55AW55SD55
	1675
	
	950
	1600
	
	
	

	1½" (40)
	AT160SR5

AT160SD5
	705
	470
	
	
	441
	106
	
	10"(250)
	AW35D004
	1612
	
	800
	320
	1187
	336
	

	
	AT140DRO

AT140DDO
	683
	405
	
	
	
	
	
	
	AW65SR55AW65SD55
	1910
	
	950
	1600
	
	
	

	2" (50)
	AT190SR5

AT190SD5
	768
	540
	
	
	492
	106
	
	12"(300)
	AW55D005
	1932
	
	950
	370
	1238
	427
	

	
	AT140DRO

AT140DDO
	700
	405
	
	
	
	
	
	
	AW65SR55AW65SD55
	1978
	
	950
	1600
	
	
	

	
	AW22SR51 AW22SD51
	822
	
	520
	910
	
	
	
	
	
	
	
	
	
	
	
	

	2½" (65)
	AT210SR5

AT210SD5
	875
	560
	
	
	530
	134
	
	14"(350)
	AW60D005
	2143
	
	950
	370
	1289
	463
	

	
	AT160DRO

AT160DDO
	807
	470
	
	
	
	
	
	
	AW65SR55AW65SD55
	2168
	
	950
	1600
	
	
	

	
	AW27SR52 AW27SD52
	964
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	

	3" (80)
	AT190DRO

AT190DDO
	941
	540
	
	
	\556
	144


	
	16"(400)
	AW60D005
	2346
	
	950
	370
	1391
	541
	

	
	AT240SR5

AT240SD5
	1000
	620
	
	
	
	
	
	
	AW65SR55AW65SD55
	2371
	
	950
	1600
	
	
	

	
	AW27SR52 AW27SD52
	1032
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	


注：结构长度A已包含袖管尺寸。

Note: Structure length A has included the sleeve size.

表4-11 上装式低温球阀 PN150/Class900配气动执行机构外形尺寸及重量（R100—300、R100—301）    mm

Table 4-11 Overall Dimensions and Weight of Top-mounted Cryogenic Ball Valve PN150/Class900 with Pneumatic Actuator (R100—300, R100—301)                                    mm

	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg
	公称通径

Nominal Diameter

Inch (mm)
	执行机构

Actuator
	H
	B
	B1
	B2
	对接焊A

Butt welding A
	H1
	重量

Weight

Kg

	1/2" (15)
	AT140SR5

AT140SD5
	572
	405
	
	
	454
	65
	
	4" (100)
	AT240DROAT240DDO
	1199
	620
	
	
	657
	183
	

	
	AT105DRO

AT105DDO
	533
	285
	
	
	
	
	
	
	AT270SR5

AT270SD5
	1238
	740
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW32SR53 AW32SD53
	1253
	
	700
	1160
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW27D002
	1254
	
	650
	250
	
	
	

	3/4" (20)
	AT140SR5

AT140SD5
	572
	405
	
	
	454
	65
	
	5" (125)
	AT240DROAT240DDO
	1349
	620
	
	
	759
	250
	

	
	AT105DRO

AT105DDO
	533
	285
	
	
	
	
	
	
	AW27D002
	1324
	
	650
	250
	
	
	

	
	
	
	
	
	
	
	
	
	
	AW40SR53 AW40SD53
	1420
	
	700
	1160
	
	
	

	1" (25)
	AT140SR5

AT140SD5
	622
	405
	
	
	454
	75
	
	6" (150)
	AW30D003
	1343
	
	700
	270
	810
	260
	

	
	AT105DRO

AT105DDO
	566
	285
	
	
	
	
	
	
	AW45SR53

AW45SD53
	1442
	
	700
	1250
	
	
	

	1¼" (32)
	AT160SR5

AT160SD5
	727
	470
	
	
	479
	90
	
	8" (200)
	AW35D004
	1470
	
	800
	320
	1137
	310
	

	
	AT125DRO

AT125DDO
	685
	285
	
	
	
	
	
	
	AW55SR55

AW55SD55
	1695
	
	950
	1600
	
	
	

	1½" (40)
	AT190SR5

AT190SD5
	810
	540
	
	
	505
	110
	
	10"(250)
	AW55D005
	1845
	
	950
	370
	1238
	3380
	

	
	AT140DRO

AT140DDO
	742
	405
	
	
	
	
	
	
	AW65SR55

AW65SD55
	1918
	
	950
	1600
	
	
	

	2" (50)
	AT210SR5

AT210SD5
	915
	560
	
	
	568
	140
	
	12"(300)
	AW60D005
	1963
	
	950
	370
	1365
	420
	

	
	AT160DRO

AT160DDO
	847
	470
	
	
	
	
	
	
	AW65SR55

AW65SD55
	1988
	
	950
	1600
	
	
	

	2½" (65)
	AT240SR5

AT240SD5
	1009
	620
	
	
	619
	150
	
	14"(350)
	AW60D005
	2196
	
	950
	370
	1429
	460
	

	
	AT190DRO

AT190DDO
	950
	540
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2221
	
	950
	1600
	
	
	

	3" (80)
	AT210DRO

AT210DDO
	1115
	560
	
	
	\581
	160


	
	16"(400)
	AW60D005
	2346
	
	950
	370
	1530
	460
	

	
	AT270SR5

AT270SD5
	1188
	740
	
	
	
	
	
	
	AW65SR55

AW65SD55
	2371
	
	950
	1600
	
	
	

	
	AW27SR52 AW27SD52
	1204
	
	650
	950
	
	
	
	
	
	
	
	
	
	
	
	


注：结构长度A已包含袖管尺寸。Note: Structure length A has included the sleeve size.
表4-12 上装式低温球阀 PN260/Class1500配气动执行机构外形尺寸及重量（R100—300、R100—301）    mm

Table 4-12 Overall Dimensions and Weight of Top-mounted Cryogenic Ball Valve PN260/Class1500 with Pneumatic Actuator (R100—300, R100—301)                                    mm

	公称通径
Inch (mm)
	执行机构
	H
	B
	B1
	B2
	对接焊A
	H1
	重量

kg

	1/2" (15)
	AT125DRO、AT125DDO
	528
	350
	
	
	457
	84
	

	
	AT160SR5、

AT160SD5
	560
	470
	
	
	
	
	

	3/4" (20)
	AT125DRO、AT125DDO
	528
	350
	
	
	457
	84
	

	
	AT160SR5、

AT160SD5
	560
	470
	
	
	
	
	

	1" (25)
	AT125DRO、AT125DDO
	528
	350
	
	
	457
	84
	

	
	AT160SR5、

AT160SD5
	560
	470
	
	
	
	
	

	1¼" (32)
	AT140DRO、AT140DDO
	603
	405
	
	
	482
	91
	

	
	AT190SR5、

AT190SD5
	658
	540
	
	
	
	
	

	1½" (40)
	AT160DRO、AT160DDO
	640
	470
	
	
	508
	94
	

	
	AT210SR5、

AT210SD5
	700
	560
	
	
	
	
	

	2" (50)
	AT240SR5

AT240SD5
	1015
	620
	
	
	568
	190
	

	
	AT190DRO

AT190DDO
	947
	540
	
	
	
	
	

	2½" (65)
	AT270SR5

AT270SD5
	1109
	740
	
	
	619
	200
	

	
	AT210DRO

AT210DDO
	1050
	560
	
	
	
	
	

	3" (80)
	AT270DRO

AT270DDO
	1215
	740
	
	
	670
	210
	

	
	AW40SR53、 AW40SD53
	1373
	
	700
	1160
	
	
	

	4" (100)
	AW40SR53 、AW40SD53
	1403
	
	700
	1160
	746
	233
	

	
	AT270DRO

AT270DDO
	1336
	740
	
	
	
	
	

	
	AW45SR53

AW45SD53
	1450
	
	700
	1250
	
	
	

	6" (150)
	AW55SR55

AW55SD55
	1595
	
	950
	1600
	905
	310
	

	
	AW35D004
	1540
	
	800
	320
	
	
	

	8" (200)
	AW65SR55

AW65SD55
	1574
	
	950
	1600
	1232
	360
	

	
	AW55D005
	1795
	
	950
	370
	
	
	

	10"(250)
	AW65SR55

AW65SD55
	1811
	
	950
	1600
	1391
	430
	

	
	AW55D005
	2071
	
	950
	370
	
	
	

	12"(300)
	AW65SR55

AW65SD55
	2007
	
	950
	1600
	1530
	471
	

	
	AW60D005
	2077
	
	950
	370
	
	
	


注：结构长度A已包含袖管尺寸。

Note: Structure length A has included the sleeve size.
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